#### Preview Changes

No of bytes that will be Programmed
Choose configuration file(.bin)

#### Device Management

Select LAN78XX
Auto Identified Part Number
Config Mode
Config Memory
EEPROM OTP
Configuration loaded from OTP byte offset

#### MAC Address

MAC Address

#### Device Identification

Device Descriptor

Vendor ID (hex)
0x
Product ID (hex)
0x
bcdDevice (bcd)
0x

String Descriptors

Language ID (hex)
0x
Manufacturer Name
Product Name
Serial Number
Configuration String
Interface String

#### Remote Wakeup and Power

Remote Wakeup
Self Power
HS Max Power
mA
FS Max Power
mA
SS Max Power
mA

#### Interrupt Endpoint bInterval

Full Speed
0x
High Speed
0x
Super Speed
0x

#### LED Configuration

##### LED 0

Enable LED 0
LED Control 0
LED 0 combine feature
enable disable
LED 0
Blink Pulse-Stretch

##### LED 1

Enable LED 1
LED Control 1
LED 1 combine featue
enable disable
LED 1
Blink Pulse-Stretch

##### LED 2

Enable LED 2
LED Control 2
LED 2 combine featue
enable disable
LED 2
Blink Pulse-Stretch

##### LED 3

Enable LED 3
LED Control 3
LED 3 combine featue
enable disable
LED 3
Blink Pulse-Stretch

#### LED Common Features

LED Blink/Pulse-Stretch Rate
2.5-Hz blink rate/400 ms pulse-stretch 5-Hz blink rate/200 ms pulse-stretch 10-Hz blink rate/100 ms pulse-stretch 20-Hz blink rate/50 ms pulse-stretch
LED Pulsing
Normal Operation pulse with a 5-kHz,programmable duty cycle when active

#### GPIO Configuration

##### Port 1

Swap D+/D-
PHY Boost
Varisense (Squelch Tune)

##### GPIO 0

GPIO 0
enable disable
GPIO 0 Buffer
Open Drain Push Pull
GPIO 0 Direction
Input Output
GPIO 0 Wake Up
Disable Enable
GPIO 0 WakeUp Polarity
Low High
GPIO 0 Data
Set Clear

##### GPIO 1

GPIO 1
enable disable
GPIO 1 Buffer
Open Drain Push Pull
GPIO 1 Direction
Input Output
GPIO 1 Wake Up
Disable Enable
GPIO 1 WakeUp Polarity
Low High
GPIO 1 Data
Set Clear

##### GPIO 2

GPIO 2
enable disable
GPIO 2 Buffer
Open Drain Push Pull
GPIO 2 Direction
Input Output
GPIO 2 Wake Up
Disable Enable
GPIO 2 WakeUp Polarity
Low High
GPIO 2 Data
Set Clear

##### GPIO 3

GPIO 3
enable disable
GPIO 3 Buffer
Open Drain Push Pull
GPIO 3 Direction
Input Output
GPIO 3 Wake Up
Disable Enable
GPIO 3 WakeUp Polarity
Low High
GPIO 3 Data
Set Clear

##### GPIO 4

GPIO 4
enable disable
GPIO 4 Buffer
Open Drain Push Pull
GPIO 4 Direction
Input Output
GPIO 4 Wake Up
Disable Enable
GPIO 4 WakeUp Polarity
Low High
GPIO 4 Data
Set Clear

##### GPIO 5

GPIO 5
enable disable
GPIO 5 Buffer
Open Drain Push Pull
GPIO 5 Direction
Input Output
GPIO 5 Wake Up
Disable Enable
GPIO 5 WakeUp Polarity
Low High
GPIO 5 Data
Set Clear

##### GPIO 6

GPIO 6
enable disable
GPIO 6 Buffer
Open Drain Push Pull
GPIO 6 Direction
Input Output
GPIO 6 wake Up
Disable Enable
GPIO 6 WakeUp Polarity
Low High
GPIO 6 Data
Set Clear

##### GPIO 7

GPIO 7
enable disable
GPIO 7 Buffer
Open Drain Push Pull
GPIO 7 Direction
Input Output
GPIO 7 Wake Up
Disable Enable
GPIO 7 WakeUp Polarity
Low High
GPIO 7 Data
Set Clear

##### GPIO 8

GPIO 8
enable disable
GPIO 8 Buffer
Open Drain Push Pull
GPIO 8 Direction
Input Output
GPIO 8 Wake Up
Disable Enable
GPIO 8 WakeUp Polarity
Low High
GPIO 8 Data
Set Clear

##### GPIO 9

GPIO 9
enable disable
GPIO 9 Buffer
Open Drain Push Pull
GPIO 9 Direction
Input Output
GPIO 9 Wake Up
Disable Enable
GPIO 9 WakeUp Polarity
Low High
GPIO 9 Data
Set Clear

##### GPIO 10

GPIO 10
enable disable
GPIO 10 Buffer
Open Drain Push Pull
GPIO 10 Direction
Input Output
GPIO 10 Wake Up
Disable Enable
GPIO 10 WakeUp Polarity
Low High
GPIO 10 Data
Set Clear

##### GPIO 11

GPIO 11
enable disable
GPIO 11 Buffer
Open Drain Push Pull
GPIO 11 Direction
Input Output
GPIO 11 Wake Up
Disable Enable
GPIO 11 WakeUp Polarity
Low High
GPIO 11 Data
Set Clear

#### Power Management

GPIO PME
disable enable
GPIO PME Configuration
Level Pulse
GPIO PME Length
Pulse Length = 1.5ms Pulse Length = 150ms
GPIO PME Polarity
Signalling Polarity Low Signalling Polarity High
GPIO Buffer Type
Open Drain Driver Push-Pull Driver
PHY Link Change
Wake up Not supported Wake up Supported
PME Packet
Packet Event Wakeup disabled Packet Event Wakeup enabled
PME Perfect DA
Perfect DA Event Wakeup disabled Perfect DA Event Wakeup enabled
GPIO Connect
disable enable
GPIO Connect Buffer Type
Open drain driver Push-Pull driver
GPIO Connect Polarity
Signalling polarity Low Signalling polarity High
PME WUFF
Wakeup Frame Detection disable Wakeup Frame Detection enable

#### Wakeup Frame Filter Configuration

Filter
disable enable
Filter Address Type
0x
Filter Pattern Offset
0x
Filter CRC 16
0x
Filter Mask Pattern [31:0]
0x
Filter Mask Pattern [63:32]
0x
Filter Mask Pattern [95:64]
0x
Filter Mask Pattern [127:96]
0x

#### Configuration Flags

Configuration Flags 0
0x
Configuration Flags 1
0x
Configuration Flags 2
0x
Configuration Flags 3
0x
Configuration Flags 4
0x
Configuration Flags 5
0x

#### Live Update (Register Read/Register Write)

Registers
LAN Registers PHY Registers
Register address(hex)
0x
Length
Register Operation
Read Write
Register value(hex)
0x

#### OTP/EEPROM Dump Memory

Choose Memory
EEPROM Memory OTP Memory
Save Dump file
Status Messages