#### Preview Changes

No of bytes that will be Programmed
Configuration Memory Usage
8KB
Configuration Memory Usage
2KB
Choose configuration file(.cfg)

#### Device Management

Select USB Hub
Auto Identified Part Number
Config Mode
Force Product
Config Memory
Firmware Memory
No of Configurations Programmed
No of Configurations Remaining
Configuration Memory Usage
8KB
Configuration Memory Usage
2KB

#### Device Identification USB 2.0

Device Descriptor

USB Vendor ID (hex)
0x
USB Product ID (hex)
0x
USB Device ID (hex)(bcdDevice)
0x
USB bcdUSB
0x

String Descriptors

Language ID (hex)
0x
Manufacturer Name
Product Name
Serial Number

#### Device Identification USB 3.1 Gen1

Device Descriptor

USB 3.1 Gen1 Vendor ID (hex)
0x
USB 3.1 Gen1 Product ID (hex)
0x
USB 3.1 Gen1Device ID (hex)(bcdDevice)
0x
USB 3.1 Gen1bcdUSB
0x

String Descriptors

Language ID (hex)
0x
Manufacturer Name
Product Name
Serial Number

Other Descriptors

UUID (hex)
0x

#### Downstream Port Configuration

##### Port 1

Swap D+/D-
PHY Boost
Varisense (Squelch Tune)

##### Port 1

USB2.0

Enable Port 1
Non-Removable Port

USB3.1 Gen 1

Enable Port 1
Non-Removable Port
Battery Charging
USB2.0 Standard USB Port-Max 500mA
USB2.0/USB3.1 Standard USB Port-Max 500mA/900mA
BC 1.2 Compliant Port-Max 1.5A
Most Devices Supported Mode-Max 2A

##### Port 2

USB2.0

Enable Port 2
Non-Removable Port

USB3.1 Gen 1

Enable Port 2
Non-Removable Port
Battery Charging
USB2.0 Standard USB Port-Max 500mA
USB2.0/USB3.1 Standard USB Port-Max 500mA/900mA
BC 1.2 Compliant Port-Max 1.5A
Most Devices Supported Mode-Max 2A

##### Port 3

USB2.0

Enable Port 3
Non-Removable Port

USB3.1 Gen 1

Enable Port 3
Non-Removable Port
Battery Charging
USB2.0 Standard USB Port-Max 500mA
USB2.0/USB3.1 Standard USB Port-Max 500mA/900mA
BC 1.2 Compliant Port-Max 1.5A
Most Devices Supported Mode-Max 2A

##### Port 4

USB2.0

Enable Port 4
Non-Removable Port

USB3.1 Gen 1

Enable Port 4
Non-Removable Port
Battery Charging
USB2.0 Standard USB Port-Max 500mA
USB2.0/USB3.1 Standard USB Port-Max 500mA/900mA
BC 1.2 Compliant Port-Max 1.5A
Most Devices Supported Mode-Max 2A

#### Downstream Port Configuration (Advanced)

##### Port 1

Swap D+/D-
PHY Boost
Varisense (Squelch Tune)

##### Port 1

Swap D+/D-
PHY Boost
Varisense (Squelch Tune)
High Speed Rise/Fall Adjust
Swap HSIC DATA/STROBE
HSIC Driver Output Impedance
Slew Tune

##### Port 2

Swap D+/D-
PHY Boost
Varisense (Squelch Tune)
High Speed Rise/Fall Adjust
Swap HSIC DATA/STROBE
HSIC Driver Output Impedance
Slew Tune

##### Port 3

Swap D+/D-
PHY Boost
Varisense (Squelch Tune)
High Speed Rise/Fall Adjust
Swap HSIC DATA/STROBE
HSIC Driver Output Impedance
Slew Tune

##### Port 4

Swap D+/D-
PHY Boost
Varisense (Squelch Tune)
High Speed Rise/Fall Adjust
Swap HSIC DATA/STROBE
HSIC Driver Output Impedance
Slew Tune

#### Upstream Port Configuration

Enable FlexConnect
Swap D+/D-
PHY Boost
Varisense (Squelch Tune)
High Speed Rise/Fall Adjust
Swap HSIC DATA/STROBE
HSIC Driver Output Impedance
Slew Tune

#### Hub Feature Controller (Internal USB Device)

Enable Feature Hub Controller

Device Descriptor

USB Vendor ID (hex)
0x
USB Product ID (hex)
0x
USB bcdDevice (hex)
0x

String Descriptors

Language ID (hex)
0x
Manufacturer Name
Product Name
Serial Number

##### Communication Device Class

Enable CDC

#### Advanced settings

Hub Power Mode
Self Power Bus Power
Hub Circuit Max Power (Self)
mA
Hub Max Power 2.0 (Self)
mA
Hub Circuit Max Power (Bus)
mA
Hub Max Power 2.0 (Bus)
mA
Hub Max Power 3.1 Gen1
mA
Upstream Charger Detection
Disabled All supported Chargers All SE1 chargers CDP charger DCP charger
SUSP_IND USB 2.0
Disable Suspend Indicator Resume Inhibit
Force Hub into Full speed mode
Reference Clock
(Default)
Reference Clock
(Target)
Enable LPM

#### Direct Register Access

Register Operation
Write Bytes Set Bits Clear Bits
Register address
0x
Register value
0x
Select file (.ini)

#### Live Update

Register address(hex)
0x
Length
Register Operation
Read Write
Register value(hex)
0x
Advanced Options
Select file (.regdmp)

#### Dump Memory

Choose Memory
Configuration Memory SPI Firmware Memory SPI Firmware with Configuration
Save Dump file

#### Flex Connect Live Update

Flexfeature
Flexfeature ON Flexfeature OFF
DCP for Downstream ports
Enable DCP Disable DCP
CHNG_PINFUNCT
Enable CHNG_PINFUNCT Disable CHNG_PINFUNCT

Enable/Disable Downstream Ports

Port 1
Enable Disable
Port 2
Enable Disable
Port 3
Enable Disable
Port 4
Enable Disable

HDD Timer

HDD Timer
None 10ms 100ms 500ms 1s 5s 10s 20s
wValue

#### Flex Connect

Enable FlexConnect

#### USB-I2C Bridge Demo

Frequency
Select I2C Operation
Read Write
Slave Address
0x
Length
Data
0x

#### USB-SPI Bridge Demo

Select SPI Operation
Read Write Transfer
Start Address
0x
Length
MOSI Data
0x
Response Count
Data
0x
MISO Data
0x
Select SPI Firmware

#### USB-GPIO Bridge Demo

PIO Number
GPIO State

#### USB-UART Bridge Demo

Baud Rate
Length
Send Data Receive Data
Status Messages