#### Device Identification USB 2.0

Device Descriptor

USB Vendor ID (hex)
0x
USB Product ID (hex)
0x
USB Device ID (hex)(bcdDevice)
0x
USB bcdUSB
0x

String Descriptors

Language ID (hex)
0x
Manufacturer Name
Product Name
Serial Number

#### Device Identification USB 3.1 Gen1

Device Descriptor

USB 3.1 Gen1 Vendor ID (hex)
0x
USB 3.1 Gen1 Product ID (hex)
0x
USB 3.1 Gen1Device ID (hex)(bcdDevice)
0x
USB 3.1 Gen1bcdUSB
0x

String Descriptors

Language ID (hex)
0x
Manufacturer Name
Product Name
Serial Number

Other Descriptors

UUID (hex)
0x

#### Downstream Port Configuration

##### Port 1

Enable Port 1
Non-Removable Port
Battery Charging
USB2.0/USB3.1 Standard USB Port-Max 500mA/900mA
BC 1.2 Compliant Port-Max 1.5A
Most Devices Supported Mode-Max 2A

##### Port 1

USB2.0

Enable Port 1
Non-Removable Port

USB3.1 Gen 1

Enable Port 1
Non-Removable Port
Battery Charging
USB2.0/USB3.1 Standard USB Port-Max 500mA/900mA
BC 1.2 Compliant Port-Max 1.5A
Most Devices Supported Mode-Max 2A

##### Port 2

USB2.0

Enable Port 2
Non-Removable Port

USB3.1 Gen 1

Enable Port 2
Non-Removable Port
Battery Charging
USB2.0/USB3.1 Standard USB Port-Max 500mA/900mA
BC 1.2 Compliant Port-Max 1.5A
Most Devices Supported Mode-Max 2A

##### Port 3

USB2.0

Enable Port 3
Non-Removable Port

USB3.1 Gen 1

Enable Port 3
Non-Removable Port
Battery Charging
USB2.0/USB3.1 Standard USB Port-Max 500mA/900mA
BC 1.2 Compliant Port-Max 1.5A
Most Devices Supported Mode-Max 2A

##### Port 4

USB2.0

Enable Port 4
Non-Removable Port

USB3.1 Gen 1

Enable Port 4
Non-Removable Port
Battery Charging
USB2.0/USB3.1 Standard USB Port-Max 500mA/900mA
BC 1.2 Compliant Port-Max 1.5A
Most Devices Supported Mode-Max 2A

##### Port 5

Port Splitting
Disable Enable
USB3 Port Power Control GPIO
GPIO 66 GPIO 5

USB2.0

Enable Port 5
Non-Removable Port

USB3.1 Gen 1

Enable Port 5
Non-Removable Port
Battery Charging
USB2.0/USB3.1 Standard USB Port-Max 500mA/900mA
BC 1.2 Compliant Port-Max 1.5A
Most Devices Supported Mode-Max 2A

##### Port 6

Port Splitting
Disable Enable
USB3 Port Power Control GPIO
GPIO 6 GPIO 4

USB2.0

Enable Port 6
Non-Removable Port

USB3.1 Gen 1

Enable Port 6
Non-Removable Port
Battery Charging
USB2.0/USB3.1 Standard USB Port-Max 500mA/900mA
BC 1.2 Compliant Port-Max 1.5A
Most Devices Supported Mode-Max 2A

##### Port 7

USB2.0

Enable Port 7
Non-Removable Port

USB3.1 Gen 1

Enable Port 7
Non-Removable Port
Battery Charging
USB2.0/USB3.1 Standard USB Port-Max 500mA/900mA
BC 1.2 Compliant Port-Max 1.5A
Most Devices Supported Mode-Max 2A

#### Downstream Port Configuration (Advanced)

##### Port 1

Swap D+/D-
PHY Boost
Varisense (Squelch Tune)

##### Port 1

Swap D+/D-
PHY Boost
Varisense (Squelch Tune)
High Speed Rise/Fall Adjust

##### Port 2

Swap D+/D-
PHY Boost
Varisense (Squelch Tune)
High Speed Rise/Fall Adjust

##### Port 3

Swap D+/D-
PHY Boost
Varisense (Squelch Tune)
High Speed Rise/Fall Adjust

##### Port 4

Swap D+/D-
PHY Boost
Varisense (Squelch Tune)
High Speed Rise/Fall Adjust

##### Port 5

Swap D+/D-
PHY Boost
Varisense (Squelch Tune)
High Speed Rise/Fall Adjust

##### Port 6

Swap D+/D-
PHY Boost
Varisense (Squelch Tune)
High Speed Rise/Fall Adjust

##### Port 7

Swap D+/D-
PHY Boost
Varisense (Squelch Tune)
High Speed Rise/Fall Adjust

##### Port Splitting(Advanced)

USB3 Port Split Link TimeOut
None 100ms 250ms 500ms 750ms 1s 2s

#### Upstream Port Configuration

Enable FlexConnect
Swap D+/D-
PHY Boost
Varisense (Squelch Tune)
High Speed Rise/Fall Adjust

#### Hub Feature Controller (Internal USB Device)

Enable Hub Feature Controller

Device Descriptor

USB Vendor ID (hex)
0x
USB Product ID (hex)
0x
USB bcdDevice (hex)
0x

String Descriptors

Language ID (hex)
0x
Manufacturer Name
Product Name
Serial Number

#### Advanced settings

Hub Power Mode
Self Power Bus Power
Hub Circuit Max Power (Self)
mA
Hub Max Power 2.0 (Self)
mA
Hub Circuit Max Power (Bus)
mA
Hub Max Power 2.0 (Bus)
mA
Hub Max Power 3.1 Gen1
mA
SUSP_IND USB 2.0
Suspend Indicator Resume Inhibit
Force Hub into Full speed mode
Enable LPM

#### Direct Register Access

Register Operation
Write Bytes Set Bits Clear Bits
Register address
0x
Register value
0x
Select file (.ini)
Status Messages