#### Preview Changes

No of bytes that will be Programmed
Configuration Memory Usage
8KB
Configuration Memory Usage
2KB
Choose configuration file(.cfg)

#### Device Management

Select USB Hub
Auto Identified Part Number
Config Mode
Force Product
Config Memory
Firmware Memory
No of Configurations Programmed
No of Configurations Remaining
Configuration Memory Usage
8KB

#### Device Identification USB 2.0

Device Descriptor

USB Vendor ID (hex)
0x
USB Product ID (hex)
0x
USB Device ID (hex)(bcdDevice)
0x
USB bcdUSB
0x

String Descriptors

Language ID (hex)
0x
Manufacturer Name
Product Name
Serial Number

#### Device Identification USB 3.1 Gen1

Device Descriptor

USB 3.1 Gen1 Vendor ID (hex)
0x
USB 3.1 Gen1 Product ID (hex)
0x
USB 3.1 Gen1Device ID (hex)(bcdDevice)
0x
USB 3.1 Gen1bcdUSB
0x

String Descriptors

Language ID (hex)
0x
Manufacturer Name
Product Name
Serial Number

Other Descriptors

UUID (hex)
0x

#### Downstream Port Configuration

##### Port 1

Enable Port 1
Non-Removable Port
Battery Charging
USB2.0/USB3.1 Standard USB Port-Max 500mA/900mA
BC 1.2 Compliant Port-Max 1.5A
Most Devices Supported Mode-Max 2A

##### Port 1

USB2.0

Enable Port 1
Non-Removable Port

USB3.1 Gen 1

Enable Port 1
Non-Removable Port
Battery Charging
USB2.0/USB3.1 Standard USB Port-Max 500mA/900mA
BC 1.2 Compliant Port-Max 1.5A
Most Devices Supported Mode-Max 2A

##### Port 2

USB2.0

Enable Port 2
Non-Removable Port

USB3.1 Gen 1

Enable Port 2
Non-Removable Port
Battery Charging
USB2.0/USB3.1 Standard USB Port-Max 500mA/900mA
BC 1.2 Compliant Port-Max 1.5A
Most Devices Supported Mode-Max 2A

##### Port 3

USB2.0

Enable Port 3
Non-Removable Port

USB3.1 Gen 1

Enable Port 3
Non-Removable Port
Battery Charging
USB2.0/USB3.1 Standard USB Port-Max 500mA/900mA
BC 1.2 Compliant Port-Max 1.5A
Most Devices Supported Mode-Max 2A

##### Port 4

USB2.0

Enable Port 4
Non-Removable Port

USB3.1 Gen 1

Enable Port 4
Non-Removable Port
Battery Charging
USB2.0/USB3.1 Standard USB Port-Max 500mA/900mA
BC 1.2 Compliant Port-Max 1.5A
Most Devices Supported Mode-Max 2A

##### Port 5

Port Splitting
Disable Enable
USB3 Port Power Control GPIO
GPIO 66 GPIO 5

USB2.0

Enable Port 5
Non-Removable Port

USB3.1 Gen 1

Enable Port 5
Non-Removable Port
Battery Charging
USB2.0/USB3.1 Standard USB Port-Max 500mA/900mA
BC 1.2 Compliant Port-Max 1.5A
Most Devices Supported Mode-Max 2A

##### Port 6

Port Splitting
Disable Enable
USB3 Port Power Control GPIO
GPIO 6 GPIO 4

USB2.0

Enable Port 6
Non-Removable Port

USB3.1 Gen 1

Enable Port 6
Non-Removable Port
Battery Charging
USB2.0/USB3.1 Standard USB Port-Max 500mA/900mA
BC 1.2 Compliant Port-Max 1.5A
Most Devices Supported Mode-Max 2A

##### Port 7

USB2.0

Enable Port 7
Non-Removable Port

USB3.1 Gen 1

Enable Port 7
Non-Removable Port
Battery Charging
USB2.0/USB3.1 Standard USB Port-Max 500mA/900mA
BC 1.2 Compliant Port-Max 1.5A
Most Devices Supported Mode-Max 2A

#### Downstream Port Configuration (Advanced)

##### Port 1

Swap D+/D-
PHY Boost
Varisense (Squelch Tune)

##### Port 1

Swap D+/D-
PHY Boost
Varisense (Squelch Tune)
High Speed Rise/Fall Adjust

##### Port 2

Swap D+/D-
PHY Boost
Varisense (Squelch Tune)
High Speed Rise/Fall Adjust

##### Port 3

Swap D+/D-
PHY Boost
Varisense (Squelch Tune)
High Speed Rise/Fall Adjust

##### Port 4

Swap D+/D-
PHY Boost
Varisense (Squelch Tune)
High Speed Rise/Fall Adjust

##### Port 5

Swap D+/D-
PHY Boost
Varisense (Squelch Tune)
High Speed Rise/Fall Adjust

##### Port 6

Swap D+/D-
PHY Boost
Varisense (Squelch Tune)
High Speed Rise/Fall Adjust

##### Port 7

Swap D+/D-
PHY Boost
Varisense (Squelch Tune)
High Speed Rise/Fall Adjust

##### Port Splitting(Advanced)

USB3 Port Split Link TimeOut
None 100ms 250ms 500ms 750ms 1s 2s

#### Upstream Port Configuration

Enable FlexConnect
Swap D+/D-
PHY Boost
Varisense (Squelch Tune)
High Speed Rise/Fall Adjust

#### Hub Controller (Internal USB Device)

Enable Hub Controller

Device Descriptor

USB Vendor ID (hex)
0x
USB Product ID (hex)
0x
USB bcdDevice (hex)
0x

String Descriptors

Language ID (hex)
0x
Manufacturer Name
Product Name
Serial Number

#### Advanced settings

Hub Power Mode
Self Power Bus Power
Hub Circuit Max Power (Self)
mA
Hub Max Power 2.0 (Self)
mA
Hub Circuit Max Power (Bus)
mA
Hub Max Power 2.0 (Bus)
mA
Hub Max Power 3.1 Gen1
mA
SUSP_IND USB 2.0
Suspend Indicator Resume Inhibit
Force Hub into Full speed mode
Reference Clock
(Default)
Reference Clock
(Target)
Enable LPM

#### Direct Register Access

Register Operation
Write Bytes Set Bits Clear Bits
Register address
0x
Register value
0x
Select file (.ini)

#### Live Update

Register address(hex)
0x
Length
Register Operation
Read Write
Register value(hex)
0x
Advanced Options
Select file (.regdmp)

#### Dump Memory

Choose Memory
Configuration Memory SPI Firmware Memory SPI Firmware with Configuration
Save Dump file

#### Flex Connect Live Update

Enable FlexConfig
Select Configuration file
Enable/Disable Flexfeature
Flexfeature ON Flexfeature OFF
HDD Timer
None 10ms 100ms 500ms 1s 5s 10s 20s
wValue

#### Flex Connect

Enable FlexConnect

#### USB-I2C Bridge Demo

Frequency
Select I2C Operation
Read Write
Slave Address
0x
Length
Data
0x

#### USB-SPI Bridge Demo

Select SPI Operation
Read Write Transfer
Start Address
0x
Length
MOSI Data
0x
Response Count
Data
0x
MISO Data
0x
Select SPI Firmware

#### USB-GPIO Bridge Demo

PIO Number
GPIO State

#### USB-UART Bridge Demo

Baud Rate
Length
Send Data Receive Data
Status Messages